libLDA(3)

$ groff -man -Tascii libLDA.3 | col -b > manual.txt

LIBLDA(3) libLDA Manual LIBLDA(3)

NAME
       LibLDA - slow control and acquisition layer for Calice’s LDA

SYNOPSIS
       #include "libLDA.hh"

       src/run/dump [-h] [OPTIONS] CONFIG
       src/run/ping [-h] [OPTIONS] CONFIG
       src/run/fifo [-h] [OPTIONS] CONFIG
       src/run/rng [-h] [OPTIONS] CONFIG
       src/run/config [-h] [OPTIONS] CONFIG
       src/run/driver [-h] [OPTIONS] CONFIG
       exemple [-h] [OPTIONS] CONFIG
       tools/utDevice [-h] [OPTIONS] CONFIG
       tools/utDaq [-h] [OPTIONS]

DESCRIPTION
       libLDA is a library that drive the LDA Calice’s devices. The library
       provides non-regression tests as dump, ping, fifo, config and driver
       and exemples executables as exemple but also utDevice and utDaq that
       extend the purpose of this library in order to drive a full Calice
       bench test.

OPTIONS
       The following options are supported:

       -c , --conf-source
      Specify the way to load configuration (default is file), among
      file, static and db.

       -p , --eth-port
      Override the ethernet port on the host specified in configura-
      tion (eth0, ...)

       -a , --lda-address
      Override the ethernet mac address specified in the config file
      (in aa:bb:cc:dd:ee:ff format)

       -v , --debug-print
      Set logging level (default: INFO) among: DEBUG, INFO, WARNING,
      ERROR, NONE

       -f , --syslog
      Use syslog instead of the standard output for log messages

       -n , --no-reinit

      Do not reinitialize LDA, DCC and DIF hardware.

       -s , --single
      Do not enter into infinite loop but do the job only once.

       -m , --mode
      Set the mode (default: 8) among: 8 (ilc-manual), 0 (ilc-auto) or
      4 (beam-test) Note: today only the beam-test is functional

       -o , --time-out
      Set the read-out trigger timeout (unit is microsecond)

       -i , --pcap-buffsize
      Set PCAP input buffer size (unit is 1Ko packet)

       -t , --trig-buffsize
      Set the read-out trigger buffer size (unit is 1 trigger)

       -d , --data-buffsize
      Set the read-out data buffer size (unit is 2 bytes)
      Note: beware that data buffer size is at less equal to the size
      of maximum event size.

       -S , --freq-slc
      Set slow control frequency (unit is Hertz)
      Note: this thread is not included into the libLDA.

       -T , --freq-slc
      Set trigger frequency (unit is Hertz)
      Note: this thread, not included in the libLDA, only run in the 8
      (ilc-manual) mode.

       -U , --freq-usr
      Set user read out frequency (unit is Hertz)
      Note: this thread is not included into the libLDA.

       -h, --help
      Print a short help text describing the supported command-line
      options, and then exit.

FILES
       data/dif-X-Y.txt
      use by exemple to write output data

       data/EE:FF:X.Y.txt
      used by utDevice and utDaqP to write the output data

REPORTING BUGS
       Please send a report to nicolas.roche@llr.in2p3.fr

AUTHORS
       Nicolas Roche, David Decotigny.

LICENCE
       This software is released under the GNU General Public License. Please
       read the COPYING file for more information.

SEE ALSO
       The full documentation for libLDA is maintained as a Latex2Html
       intranet. If a browser is installed at your site, the URL
       <http://polype/~roche/calicei/> should give you access to the complete
       manual.
       libLDA(5), calDump(1), pcat(1)

Version 1.0 August 16, 2011 LIBLDA(3)