poldhcp54

Contents

1 Introduction 1 2 Scientific Linux Cern 5.5 1

1 Introduction

poldhcp54 is an old server reconfigured with slc5.5. It is used for intensive tests using the

C++ code.

2 Scientific Linux Cern 5.5

Note that XDaq recommand 32bit OS. • Download the boot.iso.

$ md5sum /dev/sr0
eadcf980712389a687beb5df1230207c /dev/sr0

• Hit enter at welcom page • Choose “English” language • Choose “FR-latin9” keyboard • Choose “HTTP” installation method • Disable “IPv6 support” • Enter

– linuxsoft.cern.ch – /cern/slc55/i386 • Partition using default layout • Install grub on /dev/hda • Choose “Europe/Paris” using UTC • Deselect “Workstation” and select “Server” • Install “Updates” repository • Choose “Customize later” • At reboot:

– Disable “Firerwall” – Disable “SELinux”