pollinbtc

Contents

1 Introduction 1

1.1 Graphic card port . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1 1.2 Raid 0 mirroring . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1 1.3 Partitions . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1 1.4 Backups and other . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1

2 Scientific Linux Cern 5.5 2

3 Virtual machine 2

3.1 Ubuntu LTS 10.04 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2 3.2 Windows XP . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

4 svn stuffs 2

5 Xilinx tools 3

1 Introduction

pollinbtc is the new cosmic host for ehcal test bench. It is an slc5.5 embedding ubuntu

lts 10.04 and windows as virtual machines.

• eth0: BCM5761 (pci)

• eth1: BCM5764M (mother board)

$ lsb_release -a
LSB Version: :core-4.0-ia32:core-4.0-noarch:graphics-4.0-ia32:graphics-4.0-noarch:printing-4.0-ia32:printing-4.0-noarch
Distributor ID: ScientificCERNSLC
Description: Scientific Linux CERN SLC release 5.6 (Boron)
Release: 5.6
Codename: Boron

1.1 Graphic card port

Please use the dvi port on the graphic card. After installation X Desktop will be display to the first port. If you use the hdmi port using an adapter, monitor go to sleep when we start X.

1.2 Raid 0 mirroring

At boot, press F10 and next ^C to enter the SAS utility. Using this utility, create an IS volume with disk 2 and 3. This raid 0 mirror will be useful to quickly dump data from acquisition.

1.3 Partitions

# fdisk -l
...

sda1 ext2 /boot
sda2 ext3 /
sda3 swap
sda5 ext3 /home
sda6 ext3 /var
sda7 ext3 /usr/local
sdb1 ext2 /opt?

1.4 Backups and other

• /usr/local/calice/BACKUP_2011 : old stuffs • /usr/local/calice/pkg: Software packages (mostly electronic tools) • /usr/local/calice/vm: Virtuals machines • /usr/local/calice/nroche: svn configuration • /usr/local/calice/gastaldi: svn configuration • /usr/local/calice/xilinx11 : Xilinx11 software • /usr/local/calice/xilinx12 : Xilinx12 software

2 Scientific Linux Cern 5.5

Note that XDaq recommand 32bit OS. • Download the boot.iso.

$ md5sum /dev/sr0
eadcf980712389a687beb5df1230207c /dev/sr0

• type linux text at welcome page (graphic card doesn’t seems to work) • Choose “English” language • Choose “FR-latin9” keyboard • Choose “HTTP” installation method • Unseselect ipv6 support • Use this HTTP repository:

– linuxsoft.cern.ch – /cern/slc55/i386 • Choose “text mode” • Install grub boot loader in MBR: / dev/sda/ (else boot fails) • Choose “Europe/Paris” using UTC • Select “Workstation” • At reboot: use "auth config" to desable "kerbeos" and "firewall" to disable "SELinux"

3 Virtual machine

Have a look in the tools section: virtualBox.

• Default machine folder (in preferences) : /usr/local/calice/vm

3.1 Ubuntu LTS 10.04

• The iso we used is here: /usr/local/calice/vm/iso/ubuntu-10.04.2-desktop-i386.iso

3.2 Windows XP

We re-use the previous XP virtual machine.

4 svn stuffs

Have a look in the approach section: Subversion Note: there is a security process that re-arrange PATH on SLC5.6. If we want to use the icons on Desktop for SVN, in /etc/profile.d/zzz_hepix.sh:

#!/bin/sh
return # please add this line to use svn icons on desktop
...

5 Xilinx tools