Ramp

Contents

1 Introduction 1

2 Single test 1

3 Non regression test 1

1 Introduction

What: Emplementing the “config” utility that is required to test ASICs configuration and behaviour.

Binary located at:

• libLDA/run/config

This binary is used to simulate a XDAQ configuration. Note: this test shows that configuration less sometime one words.

2 Single test

# run/config poldhcp54.conf -snf

Conf ( 14): 0% [ 1,5] [ 1,8]

*** Total : miss 0 / 14 Pkts = 0%
 DIF [ 1,5] : 7 received + 0 missing 7 pkts and 0 errors.
 DIF [ 1,8] : 7 received + 0 missing 7 pkts and 0 errors.
 Dropped pkts: 0
 Unexpected pkts: 0

3 Non regression test

# run/config poldhcp54.conf -f

Flush: [buff] [ 1,5] [ 1,8]
Flush( 3): 0% 0 0
Conf ( 622): 0% [ 1,5] [ 1,8]
Conf ( 548): 0% [ 1,5] [ 1,8]
Conf ( 150): 0% [ 1,5] [ 1,8]

*** Total : miss 0 / 1323 Pkts = 0%
 DIF [ 1,5] : 660 received + 0 missing 660 pkts and 1 errors.
 DIF [ 1,8] : 660 received + 0 missing 660 pkts and 1 errors.
 Dropped pkts: 0
 Unexpected pkts: 0