Verification

Software status should be follow looking at this 4 non regression tests: Python c++ fifo (up-down links links) BT didn’t works using FC insteed of BT rng (speed download link) register order change didn’t works after a soft reset config (configure) do not use headers sometime loose the last word driver (read-out) ok ok note: fifo and rng tests only access the DIF, where config and driver tests go up to the ASICS.