Approach

Contents

1 Introduction 1 2 Generic DAQ 1 3 Harpo prototype 2

1 Introduction

This section remind the actual status and provide the methods we use to update them.

2 Generic DAQ

Online architecture is sometime done by a single framework (HESS, XDAQ) and sometime split into 3 compounds:

• Owner graphical interface • Slow control: «SLC» (Tango, ENX) wich is mainly a state machine manager. • Data aquisition: «DAQ» (Narval) wich is mainly a multiplexer also called event builder. Detector usually own 2 kind of links: • A synchronous link to the slow control • An asynchronous fast link to data aquisition

3 Harpo prototype

As the Calice’s experiment, we drive the detector using the DAQ. • We only have a synchronous link to the detector.

• Most of the embedded server functionalities have been exported to the client (DAQ).