Random generator

Contents

1 Introduction 1

2 Single test 1

3 Non regression test 1

1 Introduction

What: Emplementing the “rng” ping utility. Binary located at:

• libLDA/run/rng

This binary is used to test the downloading connection.

Note: this test shows DIF sometime doesn’t recept orders as they do not start the random packets generator..

2 Single test

# run/rng poldhcp54.conf -snf

Rng: [buff] [ 1,5] [ 1,8]
Rng ( 1): 0% 1 0

*** Total : miss 0 / 6 Pkts = 0%
 DIF [ 1,5] : 4 received + 0 missing 4 pkts and 0 errors.
 DIF [ 1,8] : 2 received + 0 missing 2 pkts and 0 errors.
 Dropped pkts: 0
 Unexpected pkts: 0

3 Non regression test

# run/rng poldhcp54.conf -f

Flush: [buff] [ 1,5] [ 1,8]
Flush( 3): 0% 0 0
Rng ( 4941): 0% 0 4941
Rng ( 4940): 0% 0 4940
Rng ( 4941): 0% 0 4941
Rng ( 575): 0% 0 575

*** Total : miss 0 / 15400 Pkts = 0%
 DIF [ 1,5] : 0 received + 0 missing 0 pkts and 0 errors.
 DIF [ 1,8] : 15397 received + 0 missing 15397 pkts and 0 errors.
 Dropped pkts: 0
 Unexpected pkts: 0